

VL HUB Update Process

1. Connect the DKT30CHPD/DKT30CHPDW to USB 3.0 host and DON'T unplug when upgdating.

2. Execute the VLI HUB FW upgrade tool, and click “Yes” to continue.



3. Firmware Update completely.



.