

**System Requirement :**

Windows OS based computer with Type-C output port

**Update Procedures :**


1. Execute the FWUpdateTool\_Setup\_V0.0.0.8.exe to install the update tool




2.Plug in the USB-C Multifunction Adapter to your computer, then click the “VL100FW Update Tool”.

You should see theCurrentVersion is 82.8.8.2 and New Version: 82.8.9.2.Then, press the "**UpdateNow**"

button to update.




3. You will see the dialog “Update OK” pop-up it means the updated successfully.



How do you verify the FW updatecompletely?

1. Unplug and re-plug in the USB-C Multifunction Adapter and press the Refresh button.


2. Check the Current Version that should be 82.8.9.2.




-------------------------------------------------------------------------------------------------------------------------------------------

Windows系統更新流程


1 . 下載JCA374更新FW之後，解壓縮之後開始安裝更軟體

2 . 按下Next直到安裝完畢



3 . 安裝完畢之後會在桌面上出現一個"VL100FWUpdateTool"請點擊執行



4 . Current Version是目前你使用的JCA374 FW版本，New Vsrsion則是你目前準備更新的FW版本

請按下Update Now直到OK更新完畢,重開機確認問題有無解決

